70802 - Deck-mounted single hole mixer with upward spout
Single hole mixer on deck with upward spout. Swivel spout, projection 250 mm, height under spout 251 mm, diameter 22 mm. 1/4 turn ceramic head with 37L/ min flow rate at 3 bar. Anti-limescale star-shaped flow straightener. Supply by PEX hoses - stainless steel braid G 1/2 '' 660 mm, withstands a temperature of 75 ° C for 30 minutes (in the context of thermal shock). Integrated non-return valves. Chromed brass body and spout. Compatible with an extension. Reference 70802, brand PRESTO or equivalent.

70802 - Deck-mounted single hole mixer with upward spout
Single hole deck mixer with upward spout, Reference 70802, brand PRESTO or equivalent, comprising:
- Swivel spout, projection 250 mm, height under spout 251 mm, diameter 22 mm
- 1/4 turn ceramic head with flow rate 37L / min at 3 bar
- Anti-limescale star-shaped flow straightener
- Supply by PEX flexible hoses - stainless steel braid G 1/2 '' 660 mm, flexible resistant to temperatures up to 75 ° C (in the context of thermal shock)
- Integrated non-return valves
- Compatible with an extension
- Chromed brass body and spout